2011-11-15 13:18:59 1 - No analysis area when analyzing 1 Water vapor H2O. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 2 - No analysis area when analyzing 2 Carbon dioxide CO2. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 3 - No analysis area when analyzing 3 Carbon monoxide CO. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 4 - No analysis area when analyzing 4 Nitrous oxide N2O. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 5 - No analysis area when analyzing 5 Nitrogen monoxide NO. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 6 - No analysis area when analyzing 6 Nitrogen dioxide NO2. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 7 - No analysis area when analyzing 7 Sulfur dioxide SO2. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 8 - No analysis area when analyzing 8 Ammonia NH3. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 9 - No analysis area when analyzing 9 Hydrogen chloride HCl. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 10 - No analysis area when analyzing 10 Hydrogen fluoride HF. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 11 - No analysis area when analyzing 11 Methane CH4. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 12 - No analysis area when analyzing 12 Ethane C2H6. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 13 - No analysis area when analyzing 13 Ethylene C2H4. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 14 - No analysis area when analyzing 14 Propane C3H8. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 15 - No analysis area when analyzing 15 Hexane C6H14. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 16 - No analysis area when analyzing 16 Formaldehyde CH2O. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 17 - No analysis area when analyzing 17 Hydrogen cyanide HCN. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 18 - No analysis area when analyzing 18 Hydrogen bromide HBr. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 19 - No analysis area when analyzing 19 Acrolein C3H4O. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 20 - No analysis area when analyzing 20 Phenol C6H6O. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 21 - No analysis area when analyzing 1 Water vapor H2O. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 22 - No analysis area when analyzing 2 Carbon dioxide CO2. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 23 - No analysis area when analyzing 3 Carbon monoxide CO. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 24 - No analysis area when analyzing 4 Nitrous oxide N2O. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 25 - No analysis area when analyzing 5 Nitrogen monoxide NO. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 26 - No analysis area when analyzing 6 Nitrogen dioxide NO2. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 27 - No analysis area when analyzing 7 Sulfur dioxide SO2. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 28 - No analysis area when analyzing 8 Ammonia NH3. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 29 - No analysis area when analyzing 9 Hydrogen chloride HCl. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 30 - No analysis area when analyzing 10 Hydrogen fluoride HF. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 31 - No analysis area when analyzing 11 Methane CH4. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 32 - No analysis area when analyzing 12 Ethane C2H6. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 33 - No analysis area when analyzing 13 Ethylene C2H4. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 34 - No analysis area when analyzing 14 Propane C3H8. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 35 - No analysis area when analyzing 15 Hexane C6H14. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 36 - No analysis area when analyzing 16 Formaldehyde CH2O. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 37 - No analysis area when analyzing 17 Hydrogen cyanide HCN. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 38 - No analysis area when analyzing 18 Hydrogen bromide HBr. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 39 - No analysis area when analyzing 19 Acrolein C3H4O. Possible reasons: Too high absorbances in sample / Bad analysis area settings
2011-11-15 13:18:59 40 - No analysis area when analyzing 20 Phenol C6H6O. Possible reasons: Too high absorbances in sample / Bad analysis area settings
